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GENERAL
SUMMARY
Section includes administrative and procedural requirements for the following:
Salvaging non-hazardous waste.
Recycling non-hazardous waste.
Disposing of non-hazardous waste.
MATERIALS OWNERSHIP
Unless otherwise indicated, construction waste becomes property of Contractor.
ACTION SUBMITTALS
Construction Waste Management Plan: Submit a project-specific Construction Waste Management Plan prior to commencement of construction activities that generate construction waste.
The Construction Waste Management Plan shall include the following:
Identification of anticipated construction waste streams generated by the Work.
Methods for salvage, recycling, and disposal of construction waste.
On-site handling, separation, storage, and transportation procedures.
Identification of responsibilities for implementation and monitoring.
Alignment of waste categories and reporting units with the UMB Construction & Demolition Waste Reporting Log. Copies are available on the Design & Construction website.
Construction activities generating construction waste shall not proceed until the Construction Waste Management Plan has been reviewed.
INFORMATIONAL SUBMITTALS
Construction Waste Reporting:
UMB Construction & Demolition Waste Reporting Log (Excel): Use the UMB  Construction & Demolition Waste Reporting Log to report construction waste generated by the Work.
Progress Submissions: Submit an updated Waste Reporting Log with each Application for Payment. Logs shall reflect cumulative construction waste quantities to date.
Supporting Documentation: Provide weight tickets, hauling manifests, receipts, invoices, or equivalent documentation supporting all reported construction waste quantities. Documentation shall identify material type, destination facility, and quantity.
Annual Waste Reports: Submit annual waste reports for multi-year projects through the end of each calendar year. Submit annual waste report by February 1 of the following year.
Final Submission: Submit a complete and final Waste Reporting Log, including all supporting documentation, prior to Substantial Completion.
Condition of Acceptance: Failure to submit accurate and complete Waste Reporting Logs may result in withholding of payment and shall delay determination of Substantial Completion.
QUALITY ASSURANCE
Waste Management Coordinator: Designate an individual responsible for implementation, monitoring, and reporting of construction waste management activities.
The Waste Management Coordinator shall:
Implement the approved Construction Waste Management Plan.
Coordinate construction waste handling practices among subcontractors.
Maintain the Waste Reporting Log and supporting documentation.
Ensure compliance with applicable laws and regulations.
Regulatory Requirements: Comply with all applicable local, state, and federal regulations governing transportation, recycling, salvage, and disposal of construction waste.
Provide relevant sustainability documentation.
PRODUCTS <Not Used>
EXECUTION
PLAN IMPLEMENTATION
Implement the approved Construction Waste Management Plan throughout the duration of the Work.
Provide containers, signage, training, handling, and transportation necessary to comply with the approved plan.
Train subcontractors and workers in proper construction waste separation and handling procedures applicable to their work.
Failure to comply with the approved Construction Waste Management Plan or reporting requirements shall be cause for corrective action and may result in withholding of payment.
SALVAGING CONSTRUCTION WASTE
Salvage construction waste designated for reuse, recycling, or donation in accordance with the approved Construction Waste Management Plan.
Handle salvaged construction waste to prevent damage, contamination, or loss.
Store salvaged construction waste in designated areas protected from weather and construction traffic.
RECYCLING CONSTRUCTION WASTE
Separate recyclable construction waste at the Project site where practical.
Transport recyclable construction waste to licensed recycling facilities capable of accepting the materials.
Do not contaminate recyclable construction waste with non-recyclable materials.
DISPOSAL OF CONSTRUCTION WASTE
Dispose of construction waste not designated for salvage or recycling at licensed, permitted disposal facilities.
Do not allow construction waste to accumulate on site except as required for orderly handling and removal.
Burning or burying of construction waste on the Project site is prohibited.
Transport construction waste in a manner that prevents spillage, dust, or contamination of adjacent areas.
END OF SECTION


CONSTRUCTION WASTE MANAGEMENT AND DISPOSAL	017419 - 1
